EVB NAME: 9002305L0-L01-04

**Misc. Notes:**

1. Artwork data supplied Gerber 274x

2. Controlled impedance requirements exist.

3. 50 Ohm micro-strip, 1 mm traces

**General Board Information:**

1. EVB board is square shaped (40mm x 40mm)
2. FR-4 Tg 150 Dk 4.2
3. Board Thickness (typ.): 0.8mm (2 layers)

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | 1 OZ finished |
| 0.8mm |  | |  |
|  |  |  | 1 OZ finished |

1. Copper finished: 1OZ
2. 2 LAYERS: TOP & BOTTOM
3. Smallest Via Size Used: 0.2 mm
4. 50 Ohms Trace width: 1 mm
5. Plating: Nickel/Gold: Ni (3 - 6um) + Au (0.075 - 0.125um)